{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["PickAndPlace_PCB_vTally_Pro_202"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"PickAndPlace_PCB_vTally_Pro_202","index":0,"n_rows":12,"n_cols":12,"rows_kept":12,"cut":false,"hidden":false,"merged":[]}
["Designator","Device","Footprint","Mid X","Mid Y","Ref X","Ref Y","Pad X","Pad Y","Layer","Rotation","SMD"]
["WEMOS_D1","WEMOS D1 RECTANGLE","WEMOS D1 RECTANGLE","42.927mm","0.763mm","54.357mm","-8.127mm","31.497mm","-8.127mm","B",90,"No"]
["MAX232","MAX232ESE","SOIC-16_L9.9-W3.9-P1.27-LS6.0-BL","46.228mm","3.683mm","46.228mm","3.683mm","41.783mm","0.947mm","T",0,"Yes"]
["R1","210Ω","R0603","32.258mm","-12.7mm","32.258mm","-12.7mm","33.011mm","-12.7mm","T",180,"Yes"]
["R2","210Ω_R0603","R0603","53.467mm","13.208mm","53.467mm","13.208mm","52.714mm","13.208mm","T",0,"Yes"]
["CAM","RC02301","RJ45-TH_RC02301","43.053mm","-9.016mm","43.053mm","-9.016mm","47.498mm","-12.951mm","T",0,"No"]
["C1","10uF","C0402","37.465mm","10.033mm","37.465mm","10.033mm","36.92mm","10.033mm","T",0,"Yes"]
["C2","10uF_C0402","C0402","38.1mm","7.493mm","38.1mm","7.493mm","37.555mm","7.493mm","T",0,"Yes"]
["C3","10uF_C0402","C0402","38.1mm","5.334mm","38.1mm","5.334mm","37.555mm","5.334mm","T",0,"Yes"]
["C4","10uF_C0402","C0402","38.1mm","3.302mm","38.1mm","3.302mm","37.555mm","3.302mm","T",0,"Yes"]
["5V","LM1117MP-5.0/TR","SOT-223-3_L6.5-W3.4-P2.30-LS7.0-BR","34.29mm","15.088mm","34.29mm","15.088mm","37.26mm","12.788mm","T",0,"Yes"]
["DC1","DC-0130-2.5A-2.5","DC-IN-TH_DC-0130-2.5A-2.5","45.517mm","11.786mm","45.517mm","11.786mm","45.767mm","9.436mm","T",270,"No"]